ContentsPreviousNext
Settings

# No Paper/Tray Not Detected (Bypass Tray)

If no paper is ready to be fed in the bypass tray, this message appears. Follow the procedure below to insert paper into the bypass tray.

Slide the bypass tray guides into position according to the paper size.

Insert a sheet of paper into the bypass tray with the print side face up.

- Support the sheet with your hands to keep it from sliding out and dropping.

- Insert the sheet straight into the bypass tray.

Press the [Test Paper Feed/Resume] key, and then push the sheet into the printer a little.

Printing starts.