ContentsPreviousNext
Settings

# Moving a Short Distance

Follow the procedure below to move the printer a short distance such as in the same room or when the options are attached.

| The printer weighs approximately 10 kg (22.1 lb.). When moving the machine, hold the machine by the bottom below the two indentations. Lift the machine slowly in order to avoid straining your body. Lifting the machine without sufficient strength or assistance or handling it roughly and dropping it could cause an injury.

| Unplug the power cord from the wall outlet before you move the machine. While moving the machine, you should take care that the power cord will not be damaged under the machine.

| When you disconnect the power plug from the wall outlet, always pull the plug (not the cable).

Turn the power off, disconnect the USB cable, and then unplug the power cord from the wall outlet.

- To make sure the print heads are capped when the machine is off, always switch the machine off from the control panel. Switching off in any other way may leave the print heads uncapped, possibly leading to printing problems.

Hold the bottom of the printer below the indents on the lower sides of the printer, and then slowly lift and move the printer without tilting it.