ContentsPreviousNext
Settings

# Print Cartridge(s) Not Detected

A Print cartridge is not installed correctly. Follow the procedure below to install the Print cartridge correctly.

1. Open the right front cover.

2. Push in the cartridge using the PUSH area.

3. Close the right front cover.

- If the error persists, take the Print cartridge out once, and then install it again. The procedure above should be performed only once.