| ContentsPreviousNext |

# Out of Printable Temperature Range

Follow the procedure below to relocate the printer when the temperature inside the printer is inappropriate, extremely high or low, for printing.

1. Turn off the power of the printer.

2. Place the printer in a 10 to 32°C (50 to 89.6°F) environment.

3. Turn on the power of the printer.

- If humidity is more than 54%, the high end of the appropriate temperature range will be lower than usual.

- Even after the power is turned on, the printer may remain in the standby mode until it acclimates to the room temperature. If this happens, wait until the [Power] key stops blinking and stays lit.

- For details about what conditions the printer can be used under (ambient temperature and humidity range), see "Checking the Installation Area", the Setup Guide.