ContentsPreviousNext
Settings

# No Paper/Tray Not Detected (Paper Tray)

No paper is loaded in the paper tray or paper is not loaded properly. Follow the procedure below to load paper properly.

1. Lift the output tray.

   When the output tray is lifted, the paper tray will pop out slightly.

2. Hold both sides of the paper tray, and pull it toward you.

   - The paper tray cannot be detached. Do not pull it forcefully.

3. Squeeze the paper guide release, and then slide the side paper guides into position according to the paper size.

   - If paper is already loaded, remove it from the paper tray, fan it well, and tap it on a flat surface such as a desk to even the edges. Check that the position of the paper guides and the front end guide match the paper size.

   - Beforehand, make sure to squeeze the front end paper guide, and then expand the guide.

4. Load paper with the print side face down but not over the limit mark.

5. Squeeze the front end paper guide, and then slide it to meet the edge of the paper.

6. Hold both sides of the paper tray, and push it gently in until it stops.

7. Lower the output tray.

8. Press the [Test Paper Feed/Resume] key.

   Printing starts.