| ContentsPreviousNext |

# Removing Paper Jammed in the Bypass Tray

Follow the procedure below to remove paper jammed in the bypass tray.

1. Remove jammed paper.

2. Press the [Test Paper Feed/Resume] key.

   - The [Test Paper Feed/Resume] key stops blinking and stays lit.

3. Insert a sheet of paper into the bypass tray with the print side face up.

4. Press the [Test Paper Feed/Resume] key.

   Printing starts.

If it is difficult to remove jammed paper, follow the procedure below to remove it.

1. Move the duplex unit locks to the unlocked position, and then detach the duplex unit (optional).

2. Remove jammed paper.

3. Attach the duplex unit (optional), and then move the duplex unit locks to the locked position.

4. Press the [Test Paper Feed/Resume] key.

   - The [Test Paper Feed/Resume] key stops blinking and stays lit.

5. Insert a sheet of paper into the bypass tray with the print side face up.

6. Press the [Test Paper Feed/Resume] key.

   Printing starts.

- When the rear cover is attached, remove the paper using the same procedure.

- Remove the rear cover if it is attached.

- Paper Is Not Fed or Delivered Normally