ContentsPreviousNext
Settings

# Printer Rear

1. USB slot

   Connect the USB cable from the computer here.

2. Power cord

   Plug the power cord into a wall outlet.

   Connect the grounding wire attached to the power plug directly to a grounding terminal.

3. Vent

   Air is vented here to prevent the inside of the printer from getting too warm. Do not lean anything against the vent or block it in any way. If the inside of the printer gets too warm, a breakdown could occur.

4. Guide board

   Open to remove paper jammed inside the printer.

5. Paper feed wheel

   Use to wind out paper jammed around the guide board.

6. Rear cover

   When paper jams around the guide board occur, detach the cover. Small items, such as booklets etc., can be place in the rear pocket.