ContentsPreviousNext
Settings

# Control Panel

1. Low ink indicators

   - The indicators correspond to the positions of the Print cartridges. From left to right, the low ink indicators display the status of the black (K), cyan (C), magenta (M), and yellow (Y) Print cartridges.

   - When an indicator is blinking, the corresponding Print cartridge is empty. Printing can continue using the ink remaining in the printer, but the Print cartridge should be replaced soon.

   - When an indicator is lit, the ink of the corresponding color has completely run out. Printing cannot be performed. The Print cartridge should be replaced immediately.

   - When all ink indicators are lit, a Print cartridge is not installed or is incorrectly installed. Make sure that the Print cartridges are correctly installed.

2. [Power] key

   - Press to turn the power on and off.

   - To turn the power on, press the key for one second until it lights.

   - After the power is turned on, the [Power] key will blink until the printer is ready for printing at which point the key will stop blinking and stay lit.

   - The [Power] key will also blink when the printer is processing data.

   - When the power is turned off, the key will blink slowly until the printer has completely shut down at which point the key will be dark.

   - When the power is off, while holding down the [Cancel] key and the [Test Paper Feed/Resume] key, press and hold down the [Power] key for over three seconds. The low ink indicators will light once and a print sample will be delivered.

   - means "standby".

3. [Test Paper Feed/Resume] key

   - Press to resume printing after dealing with an error.

   - This key lights or blinks when paper runs out or a paper jam or error occurs.

   - When using the bypass tray, press this key to start printing after inserting paper.

   - When the power is off, while holding down the [Test Paper Feed/Resume] key, press and hold down the [Power] key for over three seconds. The low ink indicators will light once and a blank sheet will be delivered.

4. [Cancel] key

   - Press to cancel printing.

   - If the [Cancel] key is pressed and held down for over three seconds, the [Power] key will blink and head cleaning will be performed for all four colors.

   - When the power is off, while holding down the [Cancel] key, press and hold down the [Power] key for over three seconds. The low ink indicators will light once and the nozzle check test pattern will be printed.