ContentsPreviousNext
Settings

# Removing Paper Jammed under the Top Cover

Follow the procedure below to remove paper jammed under the top cover.

Open the top cover.

If the carriage stops in the middle, move it to whichever side is easier to move it to.

Remove jammed paper.

- Take care not to snag the sleeves of your clothing on the cord.

- Do not touch the feed belt.

Close the top cover.

Press the [Test Paper Feed/Resume] key.

Printing starts.

- Depending on how the paper was jammed, printing may resume from the next page, not the one jammed.