ContentsPreviousNext
Settings

# Printing on Thick Paper

Follow the procedure below to print on thick paper and label paper. Thick paper and label paper are fed from the bypass tray.

- For printing using the bypass tray on paper such as thick paper, be sure to install the duplex unit (optional).

- Paper heavier than 105 g/m2 (198.5 lb.) is inserted into the bypass tray one sheet at a time. Paper lighter than that can be loaded in paper tray.

Open the printer properties dialog box from the application.

On the [Setup] tab, click [Thick] in the [Paper type:] list.

Make the necessary settings, and then click [OK].

A confirmation message appears.

Check the message, and then click [OK].

Make print settings, and then click [OK].

- The [Test Paper Feed/Resume] key lights.

Slide the envelope selector to the forward position .

Slide the bypass tray guides into position according to the paper size, and then pull the bypass tray extension out.

Insert a sheet of paper into the bypass tray with the print side face up.

- Paper can only be inserted one sheet at a time.

- Support the sheet with your hands to keep it from sliding out and dropping.

- Insert the sheet straight into the bypass tray.

- The thick paper should be between the top and bottom of the bypass tray guides.

Press the [Test Paper Feed/Resume] key, and then push the sheet into the printer a little.

Printing starts.

- Opening from an Application

- Paper Handling Precautions