*** Hints to the example program UDPExample
*** 10-02-2010

This is a Win32 Console Application.
The example program initializes all UDP or TCP data pathes and outputs the received data stream.
For more information concerning data format see the Manual Chapter Mass Data Output.

To get program options just start in a DOS box udpexample.exe without parameters.
Start the program in a DOS box with: udpexample <IP-Address>
To get the audio via LAN switch on the digital audio with the program option -am 1
For example: udpexample -am 1 89.10.11.23

You can control the instrument in parallel with any telnet application.
Command in a DOS box:  telnet <IP-Address> <Port>
For example: telnet 89.10.11.23 5555

To get scan result data choose for example the FSCAN mode with the command: freq:mode swe
and start the FSCAN with the command: init
The level measurement function is switched on after power on of the device. To enable additional 
measurement functions set the corresponding sensor functions e.g. with the command:
SENSE:FUNCTION "BANDWIDTH" or SENSE:FUNCTION "AZIMUTH"