Connect right artificial ear to analyzer input 1.
Connect left artificial ear to analyzer input 2.
Connect UPV UNBAL digital audio output to SML or SMB SPDIF input or SMBV CLK IN.
Make a suitable connection from the SMB or SML RF output to the antenna input of the DUT. 
Settings of the generator SMB or SML:
- Set frequency equal in generator and tuner
- Set RF level depending on coupling loss, e.g. -30 dBm
- Set Modulation to "Stereo"
- Deviation = 80 kHz
- Source: "Ext L,R" or "Ext S/P DIF", respectively
- Mode: R=L
- Ext L,R impedances = 100 kO
- Set Preemphasis according to regional system, matching tuner setting (50 us for Europe)
- Pilot State: On
- Pilot Deviation = 6.75 kHz
- Pilot Phase = 0 deg.
Insert earbuds into pinnas or place headphones on the HATS.
Set volume and all equalizer bands to maximum.
Start the measurement.