Connect headphones output of the player to analyzer input 1.
Connect termination resistor of 32 Ohms in parallel to the player output.
Load "ProgSimNoise-10dB.mp3" or "ProgSimNoise-10dB.wav" on player.
Set volume and all equalizer bands to maximum and start the playback.
Start the measurement.