Connect headphones to UPV generator outputs 1 and 2.
Connect right artificial ear to analyzer input 1.
Connect left artificial ear to analyzer input 2.
Insert earbud into pinna or place headphones on the HATS.
Start the measurement.