Connect right headphones output of the tuner to analyzer input 1.
Connect left headphones output of the tuner to analyzer input 2.
Connect termination resistors of 32 Ohms in parallel to the tuner outputs.
Connect UPV generator output 1 to SMB or SML modulation input.
Make a suitable connection from the SMB or SML RF output to the antenna input of the DUT. 
Settings of the generator SMB or SML:
- Set frequency equal in generator and tuner
- Set RF level depending on coupling loss, e.g. -30 dBm
- Set Modulation to "Stereo"
- Deviation = 75 kHz
- Source: "Ext L,R" or "Ext S/P DIF", respectively
- Mode: R=L
- Ext L,R impedances = 100 kO
- Set Preemphasis according to regional system, matching tuner setting (50 us for Europe)
- Pilot State: On
- Pilot Deviation = 6.75 kHz
- Pilot Phase = 0 deg.
Set volume and all equalizer bands to maximum.
Start the measurement.