Connect artificial ear to analyzer input 1.
Insert earbud into pinna or place headphones on the HATS.
Load "ProgSimNoise-10dB.mp3" or "ProgSimNoise-10dB.wav" on player.
Set volume and all equalizer bands to maximum and start the playback.
Start the measurement.