Connect right headphones output of the player to analyzer input 1.
Connect left headphones output of the player to analyzer input 2.
Connect termination resistors of 32 Ohms in parallel to the player outputs.
Load "ProgSimNoise-10dB.mp3" or "ProgSimNoise-10dB.wav" on player.
Set volume and all equalizer bands to maximum and start the playback.
Start the measurement.