Connect headphones output of the tuner to analyzer input 1.
Connect termination resistor of 32 Ohms in parallel to the tuner output.
Connect UPV generator output 1 to SMB or SML modulation input.
Make a suitable connection from the SMB or SML RF output to the antenna input of the DUT. 
Settings of the generator SMB or SML:
- Set frequency equal in generator and tuner
- Set RF level depending on coupling loss, e.g. -30 dBm
- Set Modulation to "Stereo"
- Deviation = 75 kHz
- Source: "Ext L,R" or "Ext S/P DIF", respectively
- Mode: R=L
- Ext L,R impedances = 100 kO
- Set Preemphasis according to regional system, matching tuner setting (50 us for Europe)
- Pilot State: On
- Pilot Deviation = 6.75 kHz
- Pilot Phase = 0 deg.
Set volume and all equalizer bands to maximum.
Start the measurement.