#### [SENSe<Ch>:]BANDwidth...

This subsystem sets the bandwidth of the IF measurement filter (resolution bandwidth).The forms BANDwidth and BWIDth are equivalent.

Command tree: [SENSe<Ch>:]BANDwidth|BWIDth

[:RESolution]

##### [SENSe<Ch>:]BANDwidth|BWIDth[:RESolution] <numeric_value>

Defines the resolution bandwidth of the analyzer (Meas. Bandwidth).

<Ch> | Channel number 1 to 9999. If unspecified the numeric suffix is set to 1.
<numeric_value> | Resolution bandwidth
Range [def. unit] | 1 Hz to 5 MHz [Hz]. UP and DOWN increment/decrement the bandwidth in 1-2-5 steps for each decade. The analyzer rounds up any entered value between these steps and rounds down values exceeding the maximum bandwidth.
*RST value | 10 kHz
SCPI, Command Types | Confirmed, command or query
Example: | BAND 1.1 Set a resolution bandwidth of approx. 1.1 Hz for channel 1. BAND? The analyzer returns the rounded bandwidth of 2 Hz.