### Data Transfer

The following examples show you how to perform basic tasks related to data transfer from and to the analyzer.

Copying the current setup to a floppy disk

Loading a setup stored on a floppy disk

#### To copy the active setup ...

1. Insert a floppy disk into the disk drive
   .

2. Click File — Save to open the Save As dialog.

3. Open the Save in: drop-down list and select disk drive A (labeled 3 1/2 Floppy (A)) as file location.

4. Select a File name and click Save to store the data to the disk and close the Save As dialog.

The default extension for setup files (*.zvx) is appended automatically.

#### To load a setup stored on a floppy disk...

1. Insert the floppy disk into the disk drive
   .

2. Click File — Open to open the Open dialog.

3. Open the Look in: drop-down list and select disk drive A (labeled 3 1/2 Floppy (A)) as file location.

The setup files are displayed in the center of the dialog.

1. Select a file and click Open to load the setup as the active setup.