#### [SENSe<Ch>:]LO...

This subsystem controls the Local Oscillator (LO) amplifiers for the reference and measurement channels.

Command tree: [SENSe<Ch>:]LO...

:LOMeasure

:LOReference

##### [SENSe<Ch>:]LOMeasure<Pt>[:STATe] <Boolean>

Switches the Local Oscillator amplifier for the measurement channel b on or off.

<Ch> | Channel number. If unspecified the numeric suffix is set to 1.
<Pt> | Test port number of the analyzer.
<Boolean> | ON | OFF – Switches the LO oscillator on or off.
*RST value | ON
SCPI, Command Types | Device-specific, command or query
Example: | LOM1 OFF; LOR1 OFF Switch the local oscillators for the measurement channel b and the reference channel a at port no. 1 off.

##### [SENSe<Ch>:]LOReference[:STATe] <Boolean>

Switches the Local Oscillator amplifier for the reference channel a on or off.

<Ch> | Channel number.
<Pt> | Test port number of the analyzer.
<Boolean> | ON | OFF – Switches the LO oscillator on or off.
*RST value | ON
SCPI, Command Types | Device-specific, command or query
Example: | LOM1 OFF; LOR1 OFF Switch the local oscillators for the measurement channel b and the reference channel a at port no. 1 off.