#### CALCulate<Ch>:TRANsform:VNETworks...

This subsystem defines the circuit models for single ended and balanced port (de-)embedding and activates the (de-)embedding function.

Command tree: CALCulate<Ch>:TRANsform:VNETworks

:BALanced

:DEEMbedding<Log_pt>

:PARameters

:C<nr>

:L<nr>

:R<nr>

[:STATe]

:TNDefinition

:EMBedding<Log_pt>

:PARameters

:C<nr>

:L<nr>

:R<nr>

[:STATe]

:TNDefinition

:SENDed

:DEEMbedding<Ph_pt>

:PARameters

:C<nr>

:L<nr>

:R<nr>

[:STATe]

:TNDefinition

:EMBedding<Ph_pt>

:PARameters

:C<nr>

:L<nr>

:R<nr>

[:STATe]

:TNDefinition

The circuit models are referenced by means of predefined character data parameters. They are different for single ended and balanced port (de-)embedding.

Circuit models for balanced port embedding/deembedding:

Parameter | Circuit model | Capacitances | Resistances | Inductances
FIMPort | File import, no circuit model | – | – | –
STSL | Serial Touchstone (.s2p) data, shunt L | – | R1 | L1
STSC | Serial Touchstone (.s2p) data, shunt C | C1 | R1 | –
SLST | Shunt L, serial Touchstone (.s2p) data | – | R1 | L1
SCST | Shunt C, serial Touchstone (.s2p) data | C1 | R1 | –
CSSL | Serial Cs, shunt L | C1, C2 | R1, R2, R3 | L1
LSSC | Serial Ls, shunt C | C1 | R1, R2, R3 | L1, L2
CSSC | Serial Cs, shunt C | C1, C2, C3 | R1, R2, R3 | –
LSSL | Serial Ls, shunt L | – | R1, R2, R3 | L1, L2, L3
SLCS | Shunt L, serial Cs | C1, C2 | R1, R2, R3 | L1
SCLS | Shunt C, serial Ls | C1 | R1, R2, R3 | L1, L2
SCCS | Shunt C, serial Cs | C1, C2, C3 | R1, R2, R3 | –
SLLS | Shunt L, serial Ls | – | R1, R2, R3 | L1, L2, L3

Circuit models for single ended port embedding/deembedding:

Parameter | Circuit model | Capacitances | Resistances | Inductances
FIMPort | File import, no circuit model | – | – | –
CSL | Serial C, shunt L | C1 | R1, R2 | L1
LSC | Serial L, shunt C | C1 | R1, R2 | L1
CSC | Serial C, shunt C | C1, C2 | R1, R2 | –
LSL | Serial L, shunt L | – | R1, R2 | L1, L2
SLC | Shunt L, serial C | C1 | R1, R2 | L1
SCL | Shunt C, serial L | C1 | R1, R2 | L1
SCC | Shunt C, serial C | C1, C2 | R1, R2 | –
SLL | Shunt L, serial L | – | R1, R2 | L1, L2

##### CALCulate<Ch>:TRANsform:VNETworks:BALanced:DEEMbedding<Log_pt>:PARameters:C<no>
STSC | SCST | CSSL | LSSC | CSSC | SLCS | SCLS | SCCS,<numeric_value>

Specifies the capacitance values C1, C2, C3 in the different circuit models for balanced port deembedding.

<Ch> | Channel number. If unspecified the numeric suffix is set to 1.
<Log_pt> | Logical port number
<no> | Number of capacitance in circuit model. If unspecified the numeric suffix is set to 1.
Range [def. unit] | 1 to 3 [–] The number of capacitances depends on the selected circuit model .
Parameters | Possible circuit models (character data); see circuit models .
*RST value | – (see command type description below)
<numeric_value> | Capacitance C<no> for the specified circuit model.
Range [def. unit] | –1mF to 1 mF [F]. The increment is 1 fF (10–15 F).
*RST value | 1 pF (10–12 F)
SCPI, Command Types | Device-specific, command or query. In the query form, the <numeric_value> parameter must be omitted. The command returns the capacitance value for the specified circuit model.
Example: | *RST; CALC:TRAN:VNET:BAL:DEEM:PAR:C2? CSSL Query the default capacitance C2 for the Serial Cs, shunt L circuit model. The response is 1E-012 (1 pF). CALC:TRAN:VNET:BAL:DEEM:PAR:C2 CSSL, 2.2E-12 Increase the capacitance to 2.2 pF.

##### CALCulate<Ch>:TRANsform:VNETworks:BALanced:DEEMbedding<Log_pt>:PARameters:L<no>
STSL | SLST | CSSL | LSSC | LSSL | SLCS | SCLS | SLLS,<numeric_value>

Specifies the inductance values L1, L2, L3 in the different circuit models for balanced port deembedding.

<Ch> | Channel number
<Log_pt> | Logical port number
<no> | Number of inductance in circuit model. If unspecified the numeric suffix is set to 1.
Range [def. unit] | 1 to 3 [–] The number of inductances depends on the selected circuit model .
Parameters | Possible circuit models (character data); see circuit models .
*RST value | – (see command type description below)
<numeric_value> | Inductance L<no> for the specified circuit model.
Range [def. unit] | –1H to 1 H [H]. The increment is 1 pH (10–12 H).
*RST value | 1 nH (10–9 H)
SCPI, Command Types | Device-specific, command or query. In the query form, the <numeric_value> parameter must be omitted. The command returns the inductance value for the specified circuit model.
Example: | *RST; CALC:TRAN:VNET:BAL:DEEM:PAR:L1? CSSL Query the default inductance L1 for the Serial Cs, shunt L circuit model. The response is 1E-009 (1 nH). CALC:TRAN:VNET:BAL:DEEM:PAR:L1 CSSL, 2.2E-9 Increase the inductance to 2.2 nH.

##### CALCulate<Ch>:TRANsform:VNETworks:BALanced:DEEMbedding<Log_pt>:PARameters:R<no>
STSL | STSC | SLST | SCST | CSSL | LSSC | CSSC | LSSL | SLCS | SCLS | SCCS | SLLS,<numeric_value>

Specifies the resistance values R1, R2, R3 in the different circuit models for balanced port deembedding.

<Ch> | Channel number
<Log_pt> | Logical port number
<no> | Number of resistance in circuit model. If unspecified the numeric suffix is set to 1.
Range [def. unit] | 1 to 3 [–] The number of resistances depends on the selected circuit model .
Parameters | Possible circuit models (character data); see circuit models .
*RST value | – (see command type description below)
<numeric_value> | Resistance R<no> for the specified circuit model.
Range [def. unit] | –10 MW to 10 MW [W]. The increment is 1 mW (10–3 W).
*RST value | 0 W for all resistances connected in series with an inductance 10 MW for all resistances connected in parallel with a capacitance
SCPI, Command Types | Device-specific, command or query. In the query form, the <numeric_value> parameter must be omitted. The command returns the resistance value for the specified circuit model.
Example: | *RST; CALC:TRAN:VNET:BAL:DEEM:PAR:R1? CSSL; R2? CSSL, R3? CSSL Query the default resistances for the Serial Cs, shunt L circuit model. The response is 10000000000;10000000000; 0. CALC:TRAN:VNET:BAL:DEEM:PAR:R3 CSSL, 2.2E+3 Increase the resistance R3 to 2.2 kW.

##### CALCulate<Ch>:TRANsform:VNETworks:BALanced:DEEMbedding<Log_pt>[:STATe] <Boolean>

Enables or disables the deembedding function for balanced ports. It is allowed to change the circuit model and its parameters while deembedding is enabled.

<Ch> | Channel number
<Log_pt> | Logical port number
<Boolean> | ON – Deembedding active OFF – Deembedding inactive
*RST value | OFF [–]
SCPI, Command Types | Device-specific, command or query
Example: | *RST; SOUR:LPOR1 1,2; LPOR2 3,4 Define a balanced port configuration. CALC:TRAN:VNET:BAL:DEEM:TND CSSL Select the Serial Cs, shunt L circuit model for deembedding. CALC:TRAN:VNET:BAL:DEEM:PAR:R3 CSSL, 2.2E+3; CALC:TRAN:VNET:BAL:DEEM ON Increase the resistance R3 for the Serial Cs, shunt L circuit model to 2.2 kW and enable deembedding.

##### CALCulate<Ch>:TRANsform:VNETworks:BALanced:DEEMbedding<Log_pt>:TNDefinition
FIMPort | STSL | STSC | SLST | SCST | CSSL | LSSC | CSSC | LSSL | SLCS | SCLS | SCCS | SLLS

Selects the circuit model for balanced port deembedding.

<Ch> | Channel number
<Log_pt> | Logical port number
Parameters | Possible circuit models (character data); see circuit models .
*RST value | CSSL
SCPI, Command Types | Device-specific, command or query.
Example: | See CALCulate<Ch>:TRANsform:VNETworks:BALanced:DEEMbedding[:STATe]

##### CALCulate<Ch>:TRANsform:VNETworks:BALanced:EMBedding<Log_pt>:PARameters:C<no>
STSC | SCST | CSSL | LSSC | CSSC | SLCS | SCLS | SCCS,<numeric_value>

Specifies the capacitance values C1, C2, C3 in the different circuit models for balanced port embedding.

<Ch> | Channel number
<Log_pt> | Logical port number
<no> | Number of capacitance in circuit model. If unspecified the numeric suffix is set to 1.
Range [def. unit] | 1 to 3 [–] The number of capacitances depends on the selected circuit model .
Parameters | Possible circuit models (character data); see circuit models .
*RST value | – (see command type description below)
<numeric_value> | Capacitance C<no> for the specified circuit model.
Range [def. unit] | –1mF to 1 mF [F]. The increment is 1 fF (10–15 F).
*RST value | 1 pF (10–12 F)
SCPI, Command Types | Device-specific, command or query. In the query form, the <numeric_value> parameter must be omitted. The command returns the capacitance value for the specified circuit model.
Example: | *RST; CALC:TRAN:VNET:BAL:EMB:PAR:C2? CSSL Query the default capacitance C2 for the Serial Cs, shunt L circuit model. The response is 1E-012 (1 pF). CALC:TRAN:VNET:BAL:EMB:PAR:C2 CSSL, 2.2E-12 Increase the capacitance to 2.2 pF.

##### CALCulate<Ch>:TRANsform:VNETworks:BALanced:EMBedding<Log_pt>:PARameters:L<no>
STSL | SLST | CSSL | LSSC | LSSL | SLCS | SCLS | SLLS,<numeric_value>

Specifies the inductance values L1, L2, L3 in the different circuit models for balanced port embedding.

<Ch> | Channel number
<Log_pt> | Logical port number
<no> | Number of inductance in circuit model. If unspecified the numeric suffix is set to 1.
Range [def. unit] | 1 to 3 [–] The number of inductances depends on the selected circuit model .
Parameters | Possible circuit models (character data); see circuit models .
*RST value | – (see command type description below)
<numeric_value> | Inductance L<no> for the specified circuit model.
Range [def. unit] | –1H to 1 H [H]. The increment is 1 pH (10–12 H).
*RST value | 1 nH (10–9 H)
SCPI, Command Types | Device-specific, command or query. In the query form, the <numeric_value> parameter must be omitted. The command returns the inductance value for the specified circuit model.
Example: | *RST; CALC:TRAN:VNET:BAL:EMB:PAR:L1? CSSL Query the default inductance L1 for the Serial Cs, shunt L circuit model. The response is 1E-009 (1 nH). CALC:TRAN:VNET:BAL:EMB:PAR:L1 CSSL, 2.2E-9 Increase the inductance to 2.2 nH.

##### CALCulate<Ch>:TRANsform:VNETworks:BALanced:EMBedding<Log_pt>:PARameters:R<no>
STSL | STSC | SLST | SCST | CSSL | LSSC | CSSC | LSSL | SLCS | SCLS | SCCS | SLLS,<numeric_value>

Specifies the resistance values R1, R2, R3 in the different circuit models for balanced port embedding.

<Ch> | Channel number
<Log_pt> | Logical port number
<no> | Number of resistance in circuit model. If unspecified the numeric suffix is set to 1.
Range [def. unit] | 1 to 3 [–] The number of resistances depends on the selected circuit model .
Parameters | Possible circuit models (character data); see circuit models .
*RST value | – (see command type description below)
<numeric_value> | Resistance R<no> for the specified circuit model.
Range [def. unit] | –10 MW to 10 MW [W]. The increment is 1 mW (10–3 W).
*RST value | 0 W for all resistances connected in series with an inductance 10 MW for all resistances connected in parallel with a capacitance
SCPI, Command Types | Device-specific, command or query. In the query form, the <numeric_value> parameter must be omitted. The command returns the resistance value for the specified circuit model.
Example: | *RST; CALC:TRAN:VNET:BAL:EMB:PAR:R1? CSSL; R2? CSSL, R3? CSSL Query the default resistances for the Serial Cs, shunt L circuit model. The response is 10000000000;10000000000; 0. CALC:TRAN:VNET:BAL:EMB:PAR:R3 CSSL, 2.2E+3 Increase the resistance R3 to 2.2 kW.

##### CALCulate<Ch>:TRANsform:VNETworks:BALanced:EMBedding<Log_pt>[:STATe] <Boolean>

Enables or disables the embedding function for balanced ports. It is allowed to change the circuit model and its parameters while embedding is enabled.

<Ch> | Channel number
<Log_pt> | Logical port number
<Boolean> | ON – Embedding active OFF – Embedding inactive
*RST value | OFF [–]
SCPI, Command Types | Device-specific, command or query
Example: | *RST; SOUR:LPOR1 1,2; LPOR2 3,4 Define a balanced port configuration. CALC:TRAN:VNET:BAL:EMB:TND CSSL Select the Serial Cs, shunt L circuit model for embedding. CALC:TRAN:VNET:BAL:EMB:PAR:R3 CSSL, 2.2E+3; CALC:TRAN:VNET:BAL:EMB ON Increase the resistance R3 for the Serial Cs, shunt L circuit model to 2.2 kW and enable embedding.

##### CALCulate<Ch>:TRANsform:VNETworks:BALanced:EMBedding<Log_pt>:TNDefinition
FIMPort | STSL | STSC | SLST | SCST | CSSL | LSSC | CSSC | LSSL | SLCS | SCLS | SCCS | SLLS

Selects the circuit model for balanced port embedding.

<Ch> | Channel number
<Log_pt> | Logical port number
Parameters | Possible circuit models (character data); see circuit models .
*RST value | CSSL
SCPI, Command Types | Device-specific, command or query.
Example: | See CALCulate<Ch>:TRANsform:VNETworks:BALanced:EMbedding[:STATe]

##### CALCulate<Ch>:TRANsform:VNETworks:SENDed:DEEMbedding<Ph_pt>:PARameters:C<no>
CSL | LSC | CSC | SLC | SCL | SCC,<numeric_value>

Specifies the capacitance values C1, C2 in the different circuit models for single ended port deembedding.

<Ch> | Channel number
<Ph_pt> | Physical port number
<no> | Number of capacitance in circuit model. If unspecified the numeric suffix is set to 1.
Range [def. unit] | 1 to 2 [–] The number of capacitances depends on the selected circuit model .
Parameters | Possible circuit models (character data); see circuit models .
*RST value | – (see command type description below)
<numeric_value> | Capacitance C<no> for the specified circuit model.
Range [def. unit] | –1mF to 1 mF [F]. The increment is 1 fF (10–15 F).
*RST value | 1 pF (10–12 F)
SCPI, Command Types | Device-specific, command or query. In the query form, the <numeric_value> parameter must be omitted. The command returns the capacitance value for the specified circuit model.
Example: | *RST; CALC:TRAN:VNET:SEND:DEEM:PAR:C2? CSC Query the default capacitance C2 for the Serial C, shunt C circuit model. The response is 1E-012 (1 pF). CALC:TRAN:VNET:SEND:DEEM:PAR:C2 CSC, 2.2E-12 Increase the capacitance to 2.2 pF.

##### CALCulate<Ch>:TRANsform:VNETworks:SENDed:DEEMbedding<Ph_pt>:PARameters:L<no>
CSL | LSC | LSL | SLC | SCL | SLL,<numeric_value>

Specifies the inductance values L1, L2, L3 in the different circuit models for single ended port deembedding.

<Ch> | Channel number.
<Ph_pt> | Physical port number
<no> | Number of inductance in circuit model. If unspecified the numeric suffix is set to 1.
Range [def. unit] | 1 to 3 [–] The number of inductances depends on the selected circuit model .
Parameters | Possible circuit models (character data); see circuit models .
*RST value | – (see command type description below)
<numeric_value> | Inductance L<no> for the specified circuit model.
Range [def. unit] | –1H to 1 H [H]. The increment is 1 pH (10–12 H).
*RST value | 1 nH (10–9 H)
SCPI, Command Types | Device-specific, command or query. In the query form, the <numeric_value> parameter must be omitted. The command returns the inductance value for the specified circuit model.
Example: | *RST; CALC:TRAN:VNET:SEND:DEEM:PAR:L1? SLL Query the default inductance L1 for the Shunt L, serial L circuit model. The response is 1E-009 (1 nH). CALC:TRAN:VNET:SEND:DEEM:PAR:L1 SLL, 2.2E-9 Increase the inductance to 2.2 nH.

##### CALCulate<Ch>:TRANsform:VNETworks:SENDed:DEEMbedding<Ph_pt>:PARameters:R<no>
CSL | LSC | CSC | LSL | SLC | SCL | SCC | SLL,<numeric_value>

Specifies the resistance values R1, R2, R3 in the different circuit models for single ended port deembedding.

<Ch> | Channel number.
<Ph_pt> | Physical port number
<no> | Number of resistance in circuit model. If unspecified the numeric suffix is set to 1.
Range [def. unit] | 1 to 3 [–] The number of resistances depends on the selected circuit model .
Parameters | Possible circuit models (character data); see circuit models .
*RST value | – (see command type description below)
<numeric_value> | Resistance R<no> for the specified circuit model.
Range [def. unit] | –10 MW to 10 MW [W]. The increment is 1 mW (10–3 W).
*RST value | 0 W for all resistances connected in series with an inductance 10 MW for all resistances connected in parallel with a capacitance
SCPI, Command Types | Device-specific, command or query. In the query form, the <numeric_value> parameter must be omitted. The command returns the resistance value for the specified circuit model.
Example: | *RST; CALC:TRAN:VNET:SEND:DEEM:PAR:R1? CSL; R2? CSL Query the default resistances for the Serial C, shunt L circuit model. The response is 10000000; 0. CALC:TRAN:VNET:SEND:DEEM:PAR:R2 CSL, 2.2E+3 Increase the resistance R2 to 2.2 kW.

##### CALCulate<Ch>:TRANsform:VNETworks:SENDed:DEEMbedding<Ph_pt>[:STATe] <Boolean>

Enables or disables the deembedding function for single ended ports. It is allowed to change the circuit model and its parameters while deembedding is enabled.

<Ch> | Channel number.
<Ph_pt> | Physical port number
<Boolean> | ON – Deembedding active OFF – Deembedding inactive
*RST value | OFF [–]
SCPI, Command Types | Device-specific, command or query
Example: | CALC:TRAN:VNET:SEND:DEEM:TND CSL Select the Serial C, shunt L circuit model for deembedding. CALC:TRAN:VNET:SEND:DEEM:PAR:R2 CSL, 2.2E+3; CALC:TRAN:VNET:SEND:DEEM ON Increase the resistance R2 for the Serial C, shunt L circuit model to 2.2 kW and enable deembedding.

##### CALCulate<Ch>:TRANsform:VNETworks:SENDed:DEEMbedding<Ph_pt>:TNDefinition
FIMPort | CSL | LSC | CSC | LSL | SLC | SCL | SCC | SLL

Selects the circuit model for single ended port deembedding.

<Ch> | Channel number.
<Ph_pt> | Physical port number
Parameters | Possible circuit models (character data); see circuit models .
*RST value | CSL
SCPI, Command Types | Device-specific, command or query.
Example: | See CALCulate<Ch>:TRANsform:VNETworks:SENDed:DEEMbedding[:STATe]

##### CALCulate<Ch>:TRANsform:VNETworks:SENDed:EMBedding<Ph_pt>:PARameters:C<no>
CSL | LSC | CSC | SLC | SCL | SCC,<numeric_value>

Specifies the capacitance values C1, C2 in the different circuit models for single ended port embedding.

<Ch> | Channel number.
<Ph_pt> | Physical port number
<no> | Number of capacitance in circuit model. If unspecified the numeric suffix is set to 1.
Range [def. unit] | 1 to 2 [–] The number of capacitances depends on the selected circuit model .
Parameters | Possible circuit models (character data); see circuit models .
*RST value | – (see command type description below)
<numeric_value> | Capacitance C<no> for the specified circuit model.
Range [def. unit] | –1mF to 1 mF [F]. The increment is 1 fF (10–15 F).
*RST value | 1 pF (10–12 F)
SCPI, Command Types | Device-specific, command or query. In the query form, the <numeric_value> parameter must be omitted. The command returns the capacitance value for the specified circuit model.
Example: | *RST; CALC:TRAN:VNET:SEND:EMB:PAR:C2? CSC Query the default capacitance C2 for the Serial C, shunt C circuit model. The response is 1E-012 (1 pF). CALC:TRAN:VNET:SEND:EMB:PAR:C2 CSC, 2.2E-12 Increase the capacitance to 2.2 pF.

##### CALCulate<Ch>:TRANsform:VNETworks:SENDed:EMBedding<Ph_pt>:PARameters:L<no>
CSL | LSC | LSL | SLC | SCL | SLL,<numeric_value>

Specifies the inductance values L1, L2, L3 in the different circuit models for single ended port embedding.

<Ch> | Channel number.
<Ph_pt> | Physical port number
<no> | Number of inductance in circuit model. If unspecified the numeric suffix is set to 1.
Range [def. unit] | 1 to 3 [–] The number of inductances depends on the selected circuit model .
Parameters | Possible circuit models (character data); see circuit models .
*RST value | – (see command type description below)
<numeric_value> | Inductance L<no> for the specified circuit model.
Range [def. unit] | –1H to 1 H [H]. The increment is 1 pH (10–12 H).
*RST value | 1 nH (10–9 H)
SCPI, Command Types | Device-specific, command or query. In the query form, the <numeric_value> parameter must be omitted. The command returns the inductance value for the specified circuit model.
Example: | *RST; CALC:TRAN:VNET:SEND:EMB:PAR:L1? SLL Query the default inductance L1 for the Shunt L, serial L circuit model. The response is 1E-009 (1 nH). CALC:TRAN:VNET:SEND:EMB:PAR:L1 SLL, 2.2E-9 Increase the inductance to 2.2 nH.

##### CALCulate<Ch>:TRANsform:VNETworks:SENDed:EMBedding<Ph_pt>:PARameters:R<no>
CSL | LSC | CSC | LSL | SLC | SCL | SCC | SLL,<numeric_value>

Specifies the resistance values R1, R2, R3 in the different circuit models for single ended port embedding.

<Ch> | Channel number.
<Ph_pt> | Physical port number
<no> | Number of resistance in circuit model. If unspecified the numeric suffix is set to 1.
Range [def. unit] | 1 to 3 [–] The number of resistances depends on the selected circuit model .
Parameters | Possible circuit models (character data); see circuit models .
*RST value | – (see command type description below)
<numeric_value> | Resistance R<no> for the specified circuit model.
Range [def. unit] | –10 MW to 10 MW [W]. The increment is 1 mW (10–3 W).
*RST value | 0 W for all resistances connected in series with an inductance 10 MW for all resistances connected in parallel with a capacitance
SCPI, Command Types | Device-specific, command or query. In the query form, the <numeric_value> parameter must be omitted. The command returns the resistance value for the specified circuit model.
Example: | *RST; CALC:TRAN:VNET:SEND:EMB:PAR:R1? CSL; R2? CSL Query the default resistances for the Serial C, shunt L circuit model. The response is 10000000; 0. CALC:TRAN:VNET:SEND:EMB:PAR:R2 CSL, 2.2E+3 Increase the resistance R2 to 2.2 kW.

##### CALCulate<Ch>:TRANsform:VNETworks:SENDed:EMBedding<Ph_pt>[:STATe] <Boolean>

Enables or disables the embedding function for single ended ports. It is allowed to change the circuit model and its parameters while embedding is enabled.

<Ch> | Channel number.
<Ph_pt> | Physical port number
<Boolean> | ON – Embedding active OFF – Embedding inactive
*RST value | OFF [–]
SCPI, Command Types | Device-specific, command or query
Example: | CALC:TRAN:VNET:SEND:EMB:TND CSL Select the Serial C, shunt L circuit model for embedding. CALC:TRAN:VNET:SEND:EMB:PAR:R2 CSL, 2.2E+3; CALC:TRAN:VNET:SEND:EMB ON Increase the resistance R2 for the Serial C, shunt L circuit model to 2.2 kW and enable embedding.

##### CALCulate<Ch>:TRANsform:VNETworks:SENDed:EMBedding<Ph_pt>:TNDefinition
FIMPort | CSL | LSC | CSC | LSL | SLC | SCL | SCC | SLL

Selects the circuit model for single ended port embedding.

<Ch> | Channel number.
<Ph_pt> | Physical port number
Parameters | Possible circuit models (character data); see circuit models .
*RST value | CSL
SCPI, Command Types | Device-specific, command or query.
Example: | See CALCulate<Ch>:TRANsform:VNETworks:SENDed:EMBedding[:STATe]