### Reset Values of the Status Reporting System

The table below indicates the effects of various commands upon the status reporting system of the analyzer.

Event | Switching on supply voltage Power-On-Status-Clear | DCL,SDC(Device Clear, Selected Device Clear) | *RST or SYSTem:PRESet | STATus:PRESet | *CLS
Effect | 0 | 1 |  |  |  |
Clear STB,ESR |  | yes |  |  |  | yes
Clear SRE,ESE |  | yes |  |  |  |
Clear PPE |  | yes |  |  |  |
Clear EVENt parts of the registers |  | yes |  |  |  | yes
Clear ENABle parts of all OPERation-and QUESTionable registers, Fill ENABle parts of all other registers with "1". |  | yes |  |  | yes |
Fill PTRansition parts with „1" Clear NTRansition parts |  | yes |  |  | yes |
Clear error queue | yes | yes |  |  |  | yes
Clear output buffer | yes | yes | yes | 1) | 1) | 1)
Clear command processing and input buffer | yes | yes | yes |  |  |

1) Every command being the first in a command line, i.e. immediately following a <PROGRAM MESSAGE TERMINATOR> clears the output buffer.