#### [SENSe<Ch>:]AVERage...

This subsystem sets sweep averaging parameters. The sweep average is a noise-reduction technique which consists of calculating each measurement point as an average of the same measurement point over several consecutive sweeps.

Command tree: [SENSe<Ch>:]AVERage

:COUNt

[:STATe]

:CLEar

##### [SENSe<Ch>:]AVERage:CLEar

Starts a new average cycle, clearing all previous results and thus eliminating their effect on the new cycle.

<Ch> | Channel number. If unspecified the numeric suffix is set to 1.
*RST value | –
SCPI, Command Types | Confirmed, no query
Example: | AVER:COUN 15; AVER ON Set the average factor for channel 1 to 15 and enable the sweep average. AVER:COUN 5; CLE Reduce the average factor and restart the average.

##### [SENSe<Ch>:]AVERage:COUNt <numeric_value>

Defines the number of consecutive sweeps to be combined for the sweep average (Average Factor).

<Ch> | Channel number.
<numeric_value> | Average factor
Range [def. unit] | 1 to 1000 [1]
*RST value | 10
SCPI, Command Types | Confirmed, command or query
Example: | AVER:COUN 15 Set the average factor for channel 1 to 15. AVER ON Enable the sweep average.

##### [SENSe<Ch>:]AVERage[:STATe] <Boolean>

Enable or disable the sweep average.

<Ch> | Channel number.
<Boolean> | ON | OFF - Enables or disables the automatic calculation of the sweep average over the specified number of sweeps ([SENSe<Ch>:]AVERage:COUNt ).
*RST value | ON
SCPI, Command Types | Confirmed, command or query
Example: | AVER:COUN 15 Set the average factor for channel 1 to 15. AVER ON Enable the sweep average over the defined number of sweeps.