### MEMory...

The MEMory system controls the loaded setups
of the analyzer.

The MEMory... command don't affect any stored files. Use the MEMory...
commands to store and load data and to manage files stored on a mass storage device.

Command tree: MEMory

:CATalog?

:DEFine

:DELete

:ALL

[:NAME]

:SELect

#### MEMory:CATalog?

Returns the names of all loaded setups.

Response | Comma-separated list of all setups.
*RST value | 'Set1' (the default setup is created after each *RST).
SCPI, Command Types | Confirmed (with device-specific response), query only.
Example: | `*RST; MEM:DEF 'SETUP_2'` `Create a setup named 'Setup_2' and make it the active setup.` `MEM:CAT?` `Query all setups. The response is 'Set1,Setup_2'.` `M`MEM:STOR:STAT 1, 'C:\Rohde&Schwarz\NWA\RecallSets\Setup_2.zvx'; MEM:DEL 'Setup_2.zvx' Store the active setup Setup_2 to a file, renaming it Setup_2.zvx. Close the setup.

#### MEMory:DEFine '<setup_name>'

Creates a new setup <setup_name> using default settings for the traces, channels and diagram areas. The created setup becomes the active setup.

'<setup_name>' | String parameter to specify the name of the created setup.
*RST value | –
SCPI, Command Types | Device-specific, no query.
Example: | `See MEM:CAT? .` ``

#### MEMory:DELete[:NAME] '<file_name>'

Closes the specified setup.

'<setup_name>' | String parameter to specify the name of the setup to be closed.
*RST value | –
SCPI, Command Types | Confirmed, no query.
Example: | `See MEM:CAT? .` ``

#### MEMory:SELect '<setup_name>'

Selects a setup as the active setup.

'<setup_name>' | String parameter to specify the setup.
*RST value | –
SCPI, Command Types | Device-specific, no query.
Example: | `*RST; MEM:DEF 'SETUP_2'` `Create a setup named 'Setup_2' and make it the active setup.` `MEM:SEL 'Set1'` `Activate the default setup Set1.` `M`MEM:STOR:STAT 1, 'C:\Rohde&Schwarz\NWA\RecallSets\Set1.zvx'; MEM:DEL 'Set1.zvx' Store the active setup Set1 to a file, renaming it Set1.zvx. Close the setup.