#### CALCulate<Chn>:SMOothing...

This subsystem provides the settings for trace smoothing.

Command tree: CALCulate<Chn>SMOothing

:APERture

[:STATe]

##### CALCulate<Chn>:SMOothing:APERture <numeric_value>

Defines how many measurement points are averaged to smooth the trace.

<Chn> | Channel number used to identify the active trace. If unspecified the numeric suffix is set to 1.
<numeric_value> | Smoothing aperture.
Range [def. unit] | 0.05% to 100%. A smoothing aperture of n % means that the smoothing interval for each sweep point i with stimulus value xi is equal to [xi – span*n/200, xi + span*n/200], and that the result of i is replaced by the arithmetic mean value of all measurement points in this interval. [%]
*RST value | 1
SCPI, Command Types | Device-specific, command or query.
Example: | *RST; CALC:SMO ON Activate smoothing for the default trace. CALC:SMO:APER 0.5 Reduce the smoothing aperture to 0.5 %.

##### CALCulate<Chn>:SMOothing[:STATe] <Boolean>

Enables or disables smoothing for trace no. <Chn>.

<Chn> | Channel number used to identify the active trace.
<Boolean> | ON | OFF - Smoothing on or off.
*RST value | OFF
SCPI, Command Types | Device-specific, command or query.
Example: | See CALCulate<Chn>:STATistics:SMOothing:APERture