#### CALCulate<Chn>:CLIMits...

This subsystem controls the composite limit check.

Command tree: CALCulate<Chn>:CLIMits

:FAIL?

##### CALCulate<Chn>:CLIMits:FAIL?

Returns a 0 or 1, to indicate whether or not a composite limit check on several traces has failed.

<Chn> | Channel number used to identify the active trace. This suffix is not relevant because the command provides a summary of all individual limit fails.
Response | 0 | 1 - 0 represents pass for all individual limit checks (also returned if no limit check is active at all), 1 means that the limit checks for one or more traces failed.
*RST value | 0
SCPI, Command Types | Device-specific, query only.
Example: | *RST; CALC:LIM:CONT 1 GHZ, 2 GHZ Define an upper limit line segment in the stimulus range between 1 GHz and 2 GHz, using default response values. CALC:LIM:STAT ON; FAIL? Switch the limit check on and query the result. CALC:CLIM:FAIL? Query the result for the composite limit check. As only one trace is tested, the response should be equal to the previous response..