#### CALCulate<Chn>:PHOLd

This subsystem controls the max hold (peak hold) function.

##### CALCulate<Chn>:PHOLd MAX | OFF

Enables, disables, or restarts the max hold function.

<Chn> | Channel number used to identify the active trace.
Parameters | MAX - Enable the max hold function OFF - Disables the max hold function
*RST value | OFF
SCPI, Command Types | Device-specific, command or query.
Example: | *RST; CALC:PHOL MAX Reset the instrument and enable the max hold function. CALC:PHOL OFF; PHOL MAX Restart max hold.