Gray20.dnl

This dnl file provides the 20% Flat Field signal for picture
monitor adjustment which is assigned to FLAT FIELD buttom in
1080 59.94i format.

2003.01.30

----------

Rev_CB100.dnl

This dnl file provides  100% Reverse Color Bar signal  which
is assigned to COLOR BAR button in 1080 59.94i format.

HDMB.dnl

This dnl file provides  1-30 MHz  Multiburst signal  and the
same signal with  no  chroma (Y only)  which are assigned to
MULTIBURST button in  1080 59.94i format.  These  multiburst
signals are designed for quick test from 1 to 30 MHz (0.5 to
15 MHz in chroma) with one signal.

YMB.dnl

This dnl file  provides  Y Only Multiburst signals  that are
assigned to MULTIBURST button in  1080 59.94i format.  Three
standard (pre-installed) multiburst signals  with  no chroma
(Y only) are included in the dnl file.

These supplement signals usage is not high,  so  they are in
the uncheck(e)d folder for convenience of the users who need
the signals  and  they are not pre-installed into TG700 main
frame at factory.

2002.09.12
