Gray20.dnl

This dnl file provides the 20% Flat Field signal for picture
monitor adjustment which is assigned to FLAT FIELD buttom in
525-270 format.

2003.01.30

----------

Rev75Bar.dnl

This dnl file provides 75% Reverse Color Bar signal which is
assigned to COLOR BAR button in 525-270 format.

SNG_Bar.dnl

This dnl file provides SNG Color Bar (30% Gray and SMPTE Bar
matrix) signal which is assigned to COLOR BAR button in 525-
270 format.

YMB.dnl

This dnl file  provides  Y Only Multiburst  signal  which is
assigned to MULTIBURST button in 525-270 format.

These supplement signals usage is not high,  so  they are in
the uncheck(e)d folder for convenience of the users who need
the signals  and  they are not pre-installed into TG700 main
frame at factory.

2002.09.12
