Maintain an M9 Pistol Reviews
Summary Assemble the Magazine
30 of 35
&pageText=To correctly assemble the magazine, you must:& &bulletText1= Insert the follower into the top coil of the
magazine spring.& &bulletText2= Insert the magazine spring with follower into the
magazine tube.& &bulletText3= Attach the floor plate retainer to the bottom of
the spring coil.& &bulletText4= After inserting the spring into the magazine tube,
keep tension on it with your thumb.& &bulletText5= Push and hold the magazine spring and floor
plate retainer down, and at the same time, slide
the floor plate over the sidewalls until it seats fully.& &bulletText6= Carefully insert the magazine into the pistol well.&