Maintain an M9 Pistol Reviews
Inspect for Serviceability
18 of 35
&pageText=The fourth performance measure in maintaining the M9-9mm pistol is to inspect the pistol, magazine, and ammunition for serviceability. The inspection of the M9 pistol begins with the pistol disassembled in its major components. To inspect the M9 pistol, magazine, and ammunition for serviceability, you must correctly perform each of these procedures on these major components:& &textLabel1=Slide assembly& &textLabel2=Barrel assembly& &textLabel3=Recoil spring and spring guide& &textLabel4=Receiver assembly& &textLabel5=Magazine assembly& &textLabel6=Ammunition& &textPosition=left& &mediaStyle=swf& &imageBorder=true& &enableBtns=audio&