Maintain an M9 Pistol Reviews
Summary - Disassemble the Pistol
12 of 35
&pageText=To properly disassemble the M9 pistol, you must:& &bulletText1= Let the slide go forward.& &bulletText2= Hold the M9 in a raised pistol position.& &bulletText3= Press the disassembly lever button.& &bulletText4= Rotate the disassembly lever to the down position.& &bulletText5= Remove the slide and barrel assembly from
the receiver.& &bulletText6= Compress the recoil spring and guide and remove.& &bulletText7= Separate the recoil spring from the spring guide.& &bulletText8= Push in on the locking block plunger and remove
the locking block and barrel assembly.&