Maintain an M9 Pistol Reviews
Assemble the Pistol
25 of 35
&pageText=The sixth performance measure in maintaining the M9 pistol is to assemble the pistol after it has been cleaned, inspected, and lubricated. To assemble the M9 pistol, simply reverse the procedures used to disassemble the pistol. To assemble the M9 pistol, you must correctly perform the following procedures:& &textLabel1=Grasp slide and barrel assembly& &textLabel2=Insert muzzle into the slide assembly& &textLabel3=Insert the recoil spring guide into recoil spring& &textLabel4=Insert recoil spring and guide into the recoil spring housing and seat in the cutaway on the locking block& &textLabel5=Push firing pin block lever down& &textLabel6=Grasp slide and barrel assembly and align on the receiver assembly guide rails& &textLabel7=Push slide to the rear and rotate disassembly latch lever upward& &textPosition=left& &mediaStyle=swf& &imageBorder=true& &enableBtns=audio&