Maintain an M9 Pistol Reviews
Summary - Disassemble the Magazine
13 of 35
&pageText=To properly disassemble the magazine for the M9 pistol, you must:& &bulletText1= Grasp the magazine against the palm of your hand.& &bulletText2= Depress the locking block to make the locking
block plunger protrude.& &bulletText3= Push down on the floor plate retainer stud with the
locking block plunger.& &bulletText4= Slide the floor plate forward with your thumb.& &bulletText5= Use your thumb to keep pressure on the
magazine spring.& &bulletText6= Remove the floor plate retainer, magazine spring,
and follower.& &bulletText7= Remove the magazine spring.& &bulletText8= Remove the floor plate retainer.&