Maintain an M9 Pistol Reviews
Summary Clean the Pistol and Magazine
17 of 35
&pageText=To properly clean the M9 pistol and magazine, you must:& &bulletText1= Slide assembly - clean with a cloth, use CLP on a soft
brush, and wipe dry with a clean cloth.& &bulletText2= Barrel assembly - attach a bore brush to a cleaning rod,
moisten the bore brush with CLP and insert it into the
chamber end of the barrel. Clean locking block, recoil
spring and guide with a soft brush or cloth and CLP.& &bulletText3= Receiver assembly - wipe the receiver assembly clean
with a cloth or a soft brush.& &bulletText4= Magazine - wipe the magazine tube and the follower with
CLP, a cloth, and a soft brush; and clean the magazine
spring, floor plate retainer, and floor plate with a clean cloth.& &bulletText5= Holster - remove dirt from exterior with stiff brush and
wipe interior with clean cloth.& &bulletText6= Ammunition - clean it and remove any corrosion using a
dry cloth.&