Maintain an M9 Pistol Reviews
Assemble the Magazine
27 of 35
&pageText=The last part of the sixth performance measure in maintaining the M9 pistol is to assemble the magazine after it has been cleaned, inspected, and lubricated. To assemble the magazine simply reverse the procedures used to disassemble the magazine. To assemble the magazine for the M9 pistol, you must correctly perform the following procedures:& &textLabel1=Insert follower into top coil of magazine spring& &textLabel2=Insert magazine spring and follower into magazine tube& &textLabel3=Attach and center floor plate retainer on bottom spring coil& &textLabel4=Keep tension on magazine spring with your thumb& &textLabel5=Hold magazine spring and floor plate retainer down while sliding floor plate until fully seated& &textLabel6=Carefully insert magazine into pistol well& &textPosition=left& &mediaStyle=swf& &imageBorder=true& &enableBtns=audio&