Maintain an M9 Pistol Reviews
Summary – Perform a Function Check
34 of 35
&pageText=To correctly perform a function check, you must:& &bulletText1=• Clear the pistol.& &bulletText2=• Depress the slide stop and let the slide go forward.& &bulletText3=• Insert an empty magazine into the pistol.& &bulletText4=• Retract the slide fully and release it.& &bulletText5=• Depress the magazine release button and remove
the magazine.& &bulletText6=• Place the safety lever in the SAFE position. & &bulletText7=• Depress the slide stop and let the slide go forward.& &bulletText8=• Squeeze and release the trigger.& &bulletText9=• Place the safety lever in the FIRE position.& &bulletText10=• Squeeze the trigger.& &bulletText11=• Squeeze the trigger again and hold it to the rear,
while manually retracting and releasing the slide,
and then release the trigger.& &bulletText12=• Squeeze the trigger again.&