Maintain an M9 Pistol Exercises
Summary
14 of 14
&scoringAreas=7& &label0=Cleared the pistol.& &label1=Disassembled the pistol and magazine without damaging any parts.& &label2=Cleaned the pistol, components, and ammunition.& &label3=Inspected the pistol, components, and ammunition for defects.& &label4=Lubricated the pistol and magazine correctly.& &label5=Assembled the pistol and magazine in correct sequence.& &label6=Performed a function check.& &nogo0=Failure to clear the M9 pistol results in an unsafe condition for the soldier with the pistol and those soldiers nearby.& &nogo1=Failure to disassemble the M9 pistol and magazine results in the weapon system not being able to be properly cleaned, inspected for serviceability and lubricated.& &nogo2=Failure to clean the M9 pistol and magazine results in the weapon and magazine not operating correctly when being fired.& &nogo3=Failure to inspect the M9 pistol, components, and ammunition results in the weapon becoming unserviceable or potentially dangerous to fire.& &nogo4=Failure to lubricate the M9 pistol and magazine results in the weapon not operating correctly when being fired.& &nogo5=Failure to assemble the M9 pistol and magazine results in the weapon not firing properly and presenting an unsafe situation for the soldier with the pistol and those soldiers nearby.& &nogo6=Failure to perform a function check on the M9 pistol results in the soldier with the pistol not knowing whether the weapon will function correctly and presents as unsafe situation for those soldiers nearby.& &sequence=true& &sequenceLabel=Completed tasks in the correct sequence.& &gotext=You have completed this exercise correctly. Click the Options button, select Exit and then select another task.& &nogotext=You did not complete this exercise successfully. Click the Options button, select Exit, and then select Maintain an M9 Pistol to review this material.& &enableBtns=audio&