Maintain an M240B Machine Gun Reviews
Inspect the Barrel Assembly
26 of 55
&pageText=To properly inspect the barrel assembly, you must check:& &label1=Barrel& &label2=Flash suppressor& &label3=Front sight& &label4=Carrying handle& &label5=Heat shield& &poptext1=Check barrel for bulges, bends, burrs, obstructions, or pits in chamber or bore.& &poptext2=Ensure flash suppressor is not loose.& &poptext3=Check front sight for damage or looseness.& &poptext4=Check carrying handle assembly for bent, broken, or missing parts. Slowly move barrel release to the right and ensure there are between two and seven clicks.& &poptext5=Ensure heat shield is present, undamaged, and securely attaches to barrel.&