Maintain an M240B Machine Gun Reviews
Summary – Perform a Function Check
54 of 55
&pageText=You should now be comfortable with performing a function check on your M240B after cleaning and reassembling the weapon. The eight steps to performing a function check on the M240B are:& &bulletText1=Switch safety to FIRE& &bulletText2=Pull cocking handle to rear,
return forward& &bulletText3=Close cover& &bulletText4=Switch safety to SAFE& &bulletText5=Pull trigger& &bulletText6=Switch safety to FIRE& &bulletText7=Ride bolt forward& &bulletText8=Close ejection port cover& &bulletTime1=10900& &bulletTime2=12600& &bulletTime3=18400& &bulletTime4=19900& &bulletTime5=22000& &bulletTime6=25300& &bulletTime7=27300& &bulletTime8=35500& &timedText=true& &numBullets=8& &audioXpos=320& &audioYpos=70&