Maintain an M240B Machine Gun Reviews
Quick Review 2
11 of 55
&pageText=These images represent three steps in disassembling the M240B. Match the images of each step to the descriptions on the right by dragging and dropping each image into the blank space beside the appropriate description. Left click an image to view the original images for that step. When finished, click the Next button to continue the course.& &posFeedback1=Excellent. You correctly matched the three steps to their procedures. Click the Next button to continue.& &posFeedback2=Excellent. You correctly matched the three steps to their procedures. Click the Next button to continue.& &negFeedback1=That is not correct. Study the images again or return to the review of how to disassemble the M240B machine gun, and try this Quick Review again.& &negFeedback2=You still have not mastered the steps in the disassembly of the M240B.& &link=a395p0120& &label1=Ensure the bolt is forward. Depress the locking latch and hold it in. Using the carrying handle, rotate the assembly to the upright position. Push forward, and pull the assembly out.& &label2=Depress the backplate latch, and slide the assembly straight up and away from the receiver.& &label3=Open the cover. Pull the cocking handle back to move the assembly to the rear of the receiver. Reach into the receiver and push rearward on the assembly until it is slightly out of the rear of the receiver. Grasp and remove the assembly from the receiver, and return the cocking handle forward.&