Maintain an M240B Machine Gun Reviews
Clean the Gas Regulator
20 of 55
&pageText=To properly clean the gas regulator, you must:& &label1=Clean central hole of gas regulator plug& &label2=Clean regulator plug grooves& &label3=Clean gas inlet holes& &label4=Clean surface of gas regulator plug& &label5=Clean hole in gas port bushing& &popText1=Insert the scraper into the central hole of the gas regulator, and twist clockwise until it is fully seated.& &popText2=Insert the scraper tool into the regulator plug grooves, and turn clockwise.& &popText3=Insert the small reamer into each of the gas inlet holes, and twist using hand pressure only.& &popText4=Scrape the carbon from the surface of the gas regulator plug using the tip of the scraper.& &popText5=Insert the large reamer through gas port bushing hole and twist back and forth until it enters the bore of the barrel.&