Maintain an M240B Machine Gun Reviews
Summary – Disassemble the M240B Machine Gun
12 of 55
&pageText=You should now be comfortable with the process for disassembling the M240B machine gun. To disassemble the M240B, you must:& &bulletText1=Remove barrel assembly& &bulletText2=Remove heat shield assembly& &bulletText3=Remove trigger-housing assembly& &bulletText4=Remove butt stock and buffer assembly& &bulletText5=Remove driving spring rod assembly& &bulletText6=Remove bolt and operating rod assembly& &bulletText7=Remove cover assembly& &bulletTime1=9100& &bulletTime2=11300& &bulletTime3=12800& &bulletTime4=15100& &bulletTime5=17300& &bulletTime6=19800& &bulletTime7=22300& &audioXpos=320& &audioYpos=40& &numBullets=7& &timedText=true&