Maintain an M240B Machine Gun Reviews
Replace the Bolt and Operating Rod Assembly
47 of 55
&pageText=To properly replace the bolt and operating rod assembly, you must:& &label1=Insert assembly& &label2=Push assembly into receiver& &label3=Close cover& &poptext1=Ensure bolt and operating rod are fully extended. Insert assembly into rear of receiver with bolt upward and the operating rod beneath the bolt. Ensure bolt is on top of rails located on inner walls of receiver.& &poptext2=Push entire bolt and operating rod assembly into receiver as far forward as possible. Pull trigger and allow sear to drop. Slide assembly all the way into receiver.& &poptext3=Close cover assembly, ensuring latches lock.&