1-6 Assemble the Magazine
1. Jiggle the spring and follower together.
2. Slide the base under all four tabs.
3. Clean the ammunition.
Clean the ammunition using a clean, dry cloth to wipe dirt and foriegn matter from the ammunition. Do not coat with oil.
Slide the base under all four tabs, making sure that the print is on the outside.
Jiggle the spring and follower together to install them in the magazine.