Maintain an M60 Machine Gun Reviews
Quick Review 2
20 of 44
&pageText=The six procedures for disassembling the M60 are on the screen. Determine the correct order of these six steps, and indicate your answers by dragging the numbers 1 through 6 and dropping them next to the appropriate procedure. Click the Done button to check your answers.& &posFeedback1=Excellent. You correctly determined the order of steps in the procedure for disassembling the M60 machine gun. Click the Next button to continue.& &posFeedback2=Excellent. You correctly determined the order of steps in the procedure for disassembling the M60 machine gun. Click the Next button to continue.& &negFeedback1=That is not correct. Study the images again or return to the review of how to disassemble the M60 machine gun, and try this Quick Review again.& &negFeedback2=You still have not mastered the steps in the disassembly of the M60 machine gun.& &label1=Raise the shoulder rest on the stock. Insert a pointed object into the latch hole and push it down to release the latch. Pull stock group rearward and straight away from receiver.& &label2=Remove buffer yoke and buffer. Allow driving spring guide to expand and remove buffer plunger. Remove driving spring and guide from receiver and separate. Pull charging handle to rear to separate bolt from barrel socket and return forward. Pull cam roller to start movement of bolt to rear, and push bolt rearward. Remove operating rod and bolt and separate.& &label3=Press rear of leaf spring, and rotate upward to clear sear pin. Disengage leaf spring from retaining pin. Remove retaining pin. Slide trigger mechanism forward, rotate front of the group downward, and remove it from the receiver.& &label4=Raise feed cover, unlock and remove hinge pin. Remove feed cover followed by feed tray and hanger.& &label5=Press barrel locking lever plunger, raise barrel locking lever, and pull barrel group straight out and away from receiver.& &label6=Turn receiver over. Insert pointed object, such as the cleaning rod, into latch hole and press downward to release latch. Raise rear of forearm assembly, and slide forward to remove it.& &feedbackLink=a404p0090&