Maintain an M60 Machine Gun Reviews
Perform a Function Check
41 of 44
&pageText=Once you assemble your M60, you must perform a function check to ensure the weapon is properly assembled. The nine steps to performing a function check on the M60 are:& &label1=Switch safety to FIRE& &label2=Pull charging handle to rear& &label3=Switch safety to SAFE& &label4=Return charging handle forward& &label5=Close cover& &label6=Pull trigger& &label7=Switch safety to FIRE& &label8=Pull charging handle to rear and hold& &label9=Ride bolt forward& &popText= & &popText1=Switch safety to FIRE.& &popText2=Pull charging handle back and lock bolt to rear.& &popText3=Switch safety to SAFE.& &popText4=Return charging handle to forward and locked position.& &popText5=Close cover.& &popText6=Pull trigger and ensure bolt does not go forward.& &popText7=Switch safety to FIRE.& &popText8=Pull charging handle to rear, and firmly hold in place.& &popText9=Pull trigger and gently ease bolt forward.&