Maintain an M60 Machine Gun Reviews
Remove Buffer, Operating Rod, and Bolt Assembly Group 2
15 of 44
&pageText=The second part to removing the buffer, operating rod, and bolt assembly group from the M60 is to remove the operating rod and bolt. To do this, you must:& &label1=Pull charging handle to rear and return forward& &label2=Pull cam roller until it stops& &label3=Push bolt to rear& &label4=Grasp operating rod and bolt& &label5=Remove assembly from receiver& &label6=Disengage bolt from operating rod& &popText1=Pull the charging handle to the rear to separate it from the barrel socket. Return the charging handle forward.& &popText2=Pull the cam roller until it stops.& &popText3=Push the bolt to the rear with your finger on the face of the bolt.& &popText4=Grasp the operating rod and bolt when they are about 4 inches out of the cylinder.& &popText5=Pull the operating rod and bolt from the receiver, allowing the bolt to rotate. Grasp the bolt and operating rod with both hands.& &popText6=Disengage the bolt from the operating rod by pulling forward on the operating handle and lifting upward.&