Maintain an M60 Machine Gun Exercises
Disassemble the M60 Machine Gun Exercise
4 of 10
&pageText=Now you are ready to disassemble the M60 machine gun. The six procedures for disassembling the M60 are on the screen. Determine the correct order of these six steps, and indicate your answers by dragging the numbers 1 through 6 and dropping them next to the appropriate procedure. When you have finished, click the Done button.& &posFeedback1=Correct. Click the Next button to continue.& &negFeedback2=Incorrect. Please click the Next button to continue.& &label1=Press in on the rear of the leaf spring and rotate it upward to clear if from the sear pin. Disengage the leaf spring from the front notch of the retaining pin. Remove the retaining pin by pushing it to the left. Remove the mechanism by sliding it slightly forward, rotating the front downward and removing it from the receiver.& &label2=Press the locking lever plunger to unlock the assembly. Raise the locking lever to its vertical position and remove the group by pulling straight out away from the receiver.& &label3=Turn the receiver over and insert a pointed object into the latch hole at the bottom rear of the assembly. Press downward to release the latch. Slightly raise the rear of the assembly and slide it toward the front to remove it from the receiver.&